|  |
| --- |
| **EMPTYING OF WASTE TANKS** |
|  |
| 1. | Put on essential high visibility clothing and PPE. |
| 2. | Check toilet is not in use, prop open toilet door, prop up toilet lid and check contents of waste tank. |
| 3. | Check vacuum tank assembly and hoses and start donkey engine. |
| 4. | Using the wand, stir waste holding tank contents. |
| 5. | Open valve and empty waste holding tank. |
| 6. | Close valve - replace hose and wand on vehicle - take care to avoid any spillage. |
| 7. | Fill WC holding tank with small quantity of water, then flush system to ensure system works (clean or replace filter as necessary) - then empty holding tank again. |
| 8. | Replace hose and wand on vehicle and switch off vacuum pump assembly and donkey engine. |
| 9. | Refill toilet with suitable toilet additive and fresh water mixture - flush system to ensure it works correctly. |
| 10. | Spray air freshening agent inside unit - complete service sticker/label if used. |

Disclaimer:

This document is for guidance only and should be adapted in accordance with your Company procedures.

© Portable Sanitation Europe Ltd